## WARNING This is not a toy, it is a model kit for adults. It is NOT suitable for children because it may contain dangerous small parts.

## Background Information

Model history etc

## General Instructions for PLA Models

The instructions for each step should be read carefully and assembly practiced before gluing. Some parts may need cleaning or re-adjusting before assembly. PLA model parts are normally printed on flat beds called rafts. Leave the parts on the rafts until they are needed. Remove the parts by flexing the raft and if necessary sliding the blade of a modelling knife behind the part. Be careful removing small parts this way as they may ping off. A well placed finger will prevent this. The surfaces will most likely show printing lines. Remove these by sanding lightly. Do not over sand as some parts may be hollow. Use superglue to fix the parts together. USE SUPERGLUE CAREFULLY.

## The Hull

The Hull Raft

Hull Assembly Exploded View

Hull Assembly Instructions

## The Left Track And Running Gear

The left track raft

Left Track Exploded Viee

Left Track Assembly Instructions

The right track and running gear is a mirror of the left.

## The Turret

The turret raft

The turret exploded view

Turret Assembly Instructions